# :DIFF:CWINdow

:DIFF General Commands

- :DIFF:COLor
- :DIFF:COPY
- :DIFF:CWINdow
- :DIFF:DESKew
- :DIFF:DISPlay
- :DIFF:DMODe
- :DIFF:FCHan?
- :DIFF:PATTern:FILE:GCODe
- :DIFF:PATTern:FILE:NAME
- :DIFF:PATTern:FILE:RELoad
- :DIFF:PATTern:INVert
- :DIFF:PATTern:KPATtern
- :DIFF:PATTern:MODE
- :DIFF:SCHan?
- :DIFF:SIGNal:TYPE
- :DIFF:SNOise:CALibrate
- :DIFF:SNOise:SNValue:LEVel{0:3}?
- :DIFF:STATus?
- :DIFF:TDELay
- :DIFF:UNAMe

## Command Syntax

    :DIFFN:CWINdow TIME{1:4}

Where N identifies a specific differential waveform in the form "<connection1-8>_<ch1|ch3|ch5|ch7>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1|ch3|ch5|ch7>". When two channels are paired to create a differential waveform and a common-mode waveform, the odd-numbered channel is used when specifying the waveform. For example, connection 5 differential waveform 3 (from the pairing of channels 3 and 4) is `DIFF5_3`.

## Query Syntax

    :DIFFN:CWINdow?

## Description

The `:DIFF{N}:CWINdow` command allows you to assign a differential waveform to a Waveform content window.

The `:DIFF{N}:CWINdow` command selects a Waveform content window in which to display a differential channel waveform. In Infiniium 2026, several different types of content windows exist. differential channel waveforms can only be displayed in a Waveform (`TIME`) content window of which there is currently only one available. This command is provided for future use when more than one Waveform content window is available for use.

Command Arguments and Content Windows
Argument | Displayed Waveform Content Window | Number of Available Windows | Scale Units
--- | --- | --- | ---
Programmatically | Via Front Panel
TIME{1:4} | Waveform | 4 | 4 | Y-Axis: Volts or Watts (linear scale) X-Axis: seconds