# :MEASure:HORizontal:NPERiod:NPERiods

N-Period Commands

- :MEASure:HORizontal:NPERiod
- :MEASure:HORizontal:NPERiod:EDIRection
- :MEASure:HORizontal:NPERiod:FAVorite
- :MEASure:HORizontal:NPERiod:LOCation?
- :MEASure:HORizontal:NPERiod:NPERiods
- :MEASure:HORizontal:NPERiod:OCCurrences
- :MEASure:HORizontal:NPERiod:REGion
- :MEASure:HORizontal:NPERiod:SOURce
- :MEASure:HORizontal:NPERiod:STATus?
- :MEASure:HORizontal:NPERiod:STATus:DETails?
- :MEASure:HORizontal:NPERiod:STATus:REASon?
- :MEASure:HORizontal:NPERiod:UREFerence:STATe
- :MEASure:HORizontal:NPERiod:UREFerence:VALue

## Command Syntax

    :MEASure:HORizontal:NPERiod:NPERiods <number_of_periods>

<number_of_periods> is an integer.

## Query Syntax

    :MEASure:HORizontal:NPERiod:NPERiods?

## Description

For the :MEASure:HORizontal:NPERiod measurement, specifies the number of periods to include in the measurement.

## Example Command Sequence

This sequence sets up the measurement using rising signal edges and 10 periods.

    :MEASure:HORizontal:NPERiod:SOURce CHAN1_1
    :MEASure:HORizontal:NPERiod:EDIRection RISing
    :MEASure:HORizontal:NPERiod:NPERiods 10
    //  Perform measurement
    :MEASure:HORizontal:NPERiod
    :MEASure:HORizontal:NPERiod?