# :FUNCtion:PARameters:DEMBed:CFRequency

DeEmbed (2 port) Parameters Commands

- :FUNCtion:PARameters:DEMBed:ALIGn
- :FUNCtion:PARameters:DEMBed:BANDwidth
- :FUNCtion:PARameters:DEMBed:BLIMit
- :FUNCtion:PARameters:DEMBed:BSPan?
- :FUNCtion:PARameters:DEMBed:CFRequency
- :FUNCtion:PARameters:DEMBed:FNAMe
- :FUNCtion:PARameters:DEMBed:IMPulse
- :FUNCtion:PARameters:DEMBed:MEASsim
- :FUNCtion:PARameters:DEMBed:NGAin
- :FUNCtion:PARameters:DEMBed:RCORr
- :FUNCtion:PARameters:DEMBed:RESolution
- :FUNCtion:PARameters:DEMBed:SPAN
- :FUNCtion:PARameters:DEMBed:STEP

## Command Syntax

    :FUNCtionN:PARameters:DEMBed:CFRequency <center_frequency>

Where N identifies one of up to 64 possible operators {1:64} that can be defined as part of a math function. The operators are numbered in the order that they were originally added to the function.

<center_frequency> is a double.

## Query Syntax

    :FUNCtionN:PARameters:DEMBed:CFRequency?

## Description

When the `BANDpass` filter type is selected (see `:FUNCtion:PARameters:DEMBed:BLIMit`), this command specifies the center frequency of the bandpass filter.