# :MEASure:DATA:DTIerror:EYE

Data TIE Commands

- :MEASure:DATA:DTIerror
- :MEASure:DATA:DTIerror:EYE
- :MEASure:DATA:DTIerror:FAVorite
- :MEASure:DATA:DTIerror:LOCation?
- :MEASure:DATA:DTIerror:OCCurrences
- :MEASure:DATA:DTIerror:REGion
- :MEASure:DATA:DTIerror:SOURce
- :MEASure:DATA:DTIerror:STATus?
- :MEASure:DATA:DTIerror:STATus:DETails?
- :MEASure:DATA:DTIerror:STATus:REASon?
- :MEASure:DATA:DTIerror:TIEFilter
- :MEASure:DATA:DTIerror:TIEFilter:DFACtor
- :MEASure:DATA:DTIerror:TIEFilter:SHAPe
- :MEASure:DATA:DTIerror:TIEFilter:STARt
- :MEASure:DATA:DTIerror:TIEFilter:STOP
- :MEASure:DATA:DTIerror:TIEFilter:TYPE
- :MEASure:DATA:DTIerror:UNITs
- :MEASure:DATA:DTIerror:UREFerence:STATe
- :MEASure:DATA:DTIerror:UREFerence:VALue

## Command Syntax

    :MEASure:DATA:DTIerror:EYE {EYE0 | EYE1 | EYE2}

## Query Syntax

    :MEASure:DATA:DTIerror:EYE?

## Description

If the selected signal is a PAM signal type (see the `:<source>:SIGNal:TYPE` command), this command specifies which eye threshold will be used to make the measurement.

For example, for PAM4 you can select `EYE0` for the 0/1 eye threshold, `EYE1` for the 1/2 eye threshold, or `EYE2` for the 2/3 eye threshold.