# :TRIGger:QUALify:ZONE:ZONE{N}:LOGic

:TRIGger Qualify Commands

- :TRIGger:QUALify:FOQualify
- :TRIGger:QUALify:MEASure:LLIMit
- :TRIGger:QUALify:MEASure:LOCation
- :TRIGger:QUALify:MEASure:REGion
- :TRIGger:QUALify:MEASure:ULIMit
- :TRIGger:QUALify:MODE
- :TRIGger:QUALify:STATe
- :TRIGger:QUALify:ZONE:ISZLogic
- :TRIGger:QUALify:ZONE:ZONE{N}:LOGic
- :TRIGger:QUALify:ZONE:ZONE{N}:SOURce
- :TRIGger:QUALify:ZONE:ZONE{N}:STATe
- :TRIGger:QUALify:ZONE:ZONE{N}:X
- :TRIGger:QUALify:ZONE:ZONE{N}:Y

## Command Syntax

    :TRIGger:QUALify:ZONE:ZONEN:LOGic  {AND | OR | NAND | NOR}

Where N identifies one of eight possible zones {1:8}. For example, `ZONE2`.

## Query Syntax

    :TRIGger:QUALify:ZONE:ZONEN:LOGic?

## Description

Selects the type of the specified zone and the logic used to combine other zones used for the same signal:

| "Must Intersect" | "Must Not Intersect"
--- | --- | ---
Zones for the same signal are "ANDed" | AND | NAND
Zones for the same signal are "ORed" | OR | NOR

Use the `:TRIGger:QUALify:ZONE:ZONE{N}:SOURce` command to select the signal on which the zone operates.