# :MEASure:MTESt:MHITs:STATus?

Mask Margin Violation Commands

- :MEASure:MTESt:MHITs?
- :MEASure:MTESt:MHITs:LOCation?
- :MEASure:MTESt:MHITs:STATus?
- :MEASure:MTESt:MHITs:STATus:DETails?
- :MEASure:MTESt:MHITs:STATus:REASon?

## Query Syntax

    :MEASure:MTESt{N}:MHITs:STATus?

{N} identifies a specific mask and must be a value from 1 to 16. For example, `:MTESt2` selects mask 2.

## Query Response

    {CORR | INV | QUES}

CORR
  The measurement result is correct.
INV
  The measurement result is invalid.
QUES
  The measurement result is questionable.

## Description

Queries the status of the MHITs measurement. Use the `:MEASure:MTESt:MHITs:STATus:REASon?` child query to determine the reason for an invalid or questionable measurement. Additional information about the failure may be available using the `:MEASure:MTESt:MHITs:STATus:DETails?` child query.

## See Also

- Measurement Errors