# :SOURce:JITTer:DRJ?

Simulated and AWG Commands

- :SOURce:AMPLitude
- :SOURce:CDIVide
- :SOURce:DIFFerential
- :SOURce:FILTer:CUToff
- :SOURce:FILTer:RTIMe
- :SOURce:FILTer:STATe
- :SOURce:FILTer:TYPE
- :SOURce:FNAMe
- :SOURce:FORMat
- :SOURce:FOTWo:JITTer
- :SOURce:FOTWo:STATe
- :SOURce:FUNCtion
- :SOURce:INVert
- :SOURce:JITTer:BLIMit
- :SOURce:JITTer:BLSTate
- :SOURce:JITTer:DRJ?
- :SOURce:JITTer:DRN?
- :SOURce:JITTer:RJ
- :SOURce:JITTer:STATe
- :SOURce:LEVel
- :SOURce:NOISe:RN
- :SOURce:NOISe:STATe
- :SOURce:OENable
- :SOURce:OFFSet
- :SOURce:PATTern
- :SOURce:PLENgth
- :SOURce:PWIDth
- :SOURce:SEED
- :SOURce:SKEW
- :SOURce:SRATe
- :SOURce:SSC:FREQuency
- :SOURce:SSC:PATTern
- :SOURce:SSC:PERCent
- :SOURce:SSC:PHASe
- :SOURce:SSC:PPM
- :SOURce:SSC:STATe
- :SOURce:SSC:STYPe
- :SOURce:WTYPe

## Query Syntax

    :SOURceN:JITTer:DRJ?

Where N identifies a simulated instrument's specific channel in the form "<connection1-8>_<ch1-8>" (for example, `SOURce4_2`). With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1-8>" (for example, `SOURce3` which is the same as `SOURce1_3`).

## Description

On simulated instruments, returns the amount of Resultant Random Jitter applied to a differential source waveforms. To return the Resultant Random Noise, use the `:SOURce:JITTer:DRN?` command.