# :MEASure:EYE:PAM:PPAMplitude:THRatio

:PAM Pk-Pk Amplitude Commands

- :MEASure:EYE:PAM:PPAMplitude
- :MEASure:EYE:PAM:PPAMplitude:FAVorite
- :MEASure:EYE:PAM:PPAMplitude:LOCation?
- :MEASure:EYE:PAM:PPAMplitude:SOURce
- :MEASure:EYE:PAM:PPAMplitude:STATus?
- :MEASure:EYE:PAM:PPAMplitude:STATus:DETails?
- :MEASure:EYE:PAM:PPAMplitude:STATus:REASon?
- :MEASure:EYE:PAM:PPAMplitude:THRatio
- :MEASure:EYE:PAM:PPAMplitude:UNITs

## Command Syntax

    :MEASure:EYE:PAM:PPAMplitude:THRatio <ratio>

## Query Syntax

    :MEASure:EYE:PAM:PPAMplitude:THRatio?

## Description

Enters the hit ratio used by the Pk-Pk Amplitude measurements. The default hit ratio is 1e-2 which is called out in the IEEE 802.3cu standard.