# :CGMemory:CWINdow

:CGMemory General Commands

- :CGMemory:CLEar
- :CGMemory:COLor
- :CGMemory:CWINdow
- :CGMemory:DISPlay
- :CGMemory:DSTatus?
- :CGMemory:DSTatus:REASon?
- :CGMemory:PERSistence
- :CGMemory:SIGNal:TYPE
- :CGMemory:STATus?
- :CGMemory:UNAMe
- :CGMemory:UNAMe:UFName

## Command Syntax

    :CGMemoryN:CWINdow TIME{1:4}

Where N identifies one of eight color grade memories. For example, the color grade memory 2 would be identified as :CGMemory2.

## Query Syntax

    :CGMemoryN:CWINdow?

## Description

The `:CGMemory{1:8}:CWINdow` command allows you to assign a color grade memory waveform to a Waveform content window.

Command Arguments and Content Windows
Argument | Displayed Waveform Content Window | Number of Available Windows | Scale Units
--- | --- | --- | ---
Programmatically | Via Front Panel
TIME{1:4} | Waveform | 4 | 4 | Y-Axis: Volts or Watts (linear scale) X-Axis: seconds