# :MEASure:PAM:RFTime:UREFerence:VALue

PAM Rise/Fall Times Commands

- :MEASure:PAM:RFTime
- :MEASure:PAM:RFTime:EDIRection
- :MEASure:PAM:RFTime:FAVorite
- :MEASure:PAM:RFTime:LOCation?
- :MEASure:PAM:RFTime:OCCurrences
- :MEASure:PAM:RFTime:REGion
- :MEASure:PAM:RFTime:SOURce
- :MEASure:PAM:RFTime:STATus?
- :MEASure:PAM:RFTime:STATus:DETails?
- :MEASure:PAM:RFTime:STATus:REASon?
- :MEASure:PAM:RFTime:TRANsition
- :MEASure:PAM:RFTime:UREFerence:STATe
- :MEASure:PAM:RFTime:UREFerence:VALue

## Command Syntax

    :MEASure:PAM:RFTime:UREFerence:VALue <time_location>

<time_location> is a double.

## Query Syntax

    :MEASure:PAM:RFTime:UREFerence:VALue?

## Description

When a user-defined horizontal reference location is enabled (see `:MEASure:PAM:RFTime:UREFerence:STATe`), this command specifies its time location with respect to the trigger (t = 0) location.