# :NETWorks:TRACe:XSCale?

:NETWorks:TRACe Scaling Commands

- :NETWorks:TRACe:XLEFt?
- :NETWorks:TRACe:XPOSition?
- :NETWorks:TRACe:XREFerence?
- :NETWorks:TRACe:XRIGht?
- :NETWorks:TRACe:XSCale?
- :NETWorks:TRACe:XUNits?
- :NETWorks:TRACe:YBOTtom?
- :NETWorks:TRACe:YOFFset?
- :NETWorks:TRACe:YRANge?
- :NETWorks:TRACe:YSCale?
- :NETWorks:TRACe:YTOP?
- :NETWorks:TRACe:YUNits?

## Query Syntax

    :NETWorks:TRACeN:XSCale?

Where N identifies a specific trace and must be selected from 1 to 128 {1:128}.

## Description

Queries the X-axis scale for the graph of the indicated S-parameter trace. Use the `:NETWorks:TRACe:XPOSition?` command to set or query the value at the center of the horizontal axis. You can query the value at the left side of the graph using the `:NETWorks:TRACe:XLEFt?` command. You can query the value at the ride side of the graph using the `:NETWorks:TRACe:XRIGht?` command.

Units for Displayed Content Window Graphs
Content Window Graphs | Y-Axis Units | X-Axis Units
--- | --- | ---
S-Parameters
Freq-Mag | Decibels | Hertz
Phase | Degrees
GrpDelay | Seconds