# :LTESt:ACQuire:SIMage:STATe

:LTESt Acquisition Commands

- :LTESt:ACQuire:CTYPe
- :LTESt:ACQuire:CTYPe:SAMPles
- :LTESt:ACQuire:CTYPe:WAVeforms
- :LTESt:ACQuire:SIMage:FNAMe
- :LTESt:ACQuire:SIMage:FNAMe:AUPDate
- :LTESt:ACQuire:SIMage:FNAMe:USTandard
- :LTESt:ACQuire:SIMage:FTYPe?
- :LTESt:ACQuire:SIMage:IMETadata
- :LTESt:ACQuire:SIMage:INVert
- :LTESt:ACQuire:SIMage:MONochrome
- :LTESt:ACQuire:SIMage:SINClude
- :LTESt:ACQuire:SIMage:STATe
- :LTESt:ACQuire:SIMage:WINDow
- :LTESt:ACQuire:STATe
- :LTESt:ACQuire:SWAVeform:CHANnel{N}:FNAMe
- :LTESt:ACQuire:SWAVeform:CHANnel:FTYPe
- :LTESt:ACQuire:SWAVeform:CHANnel{N}:STATe
- :LTESt:ACQuire:SWAVeform:CHANnel{N}:WMEMory
- :LTESt:ACQuire:SWAVeform:CMODe{N}:FNAMe
- :LTESt:ACQuire:SWAVeform:CMODe:FTYPe
- :LTESt:ACQuire:SWAVeform:CMODe{N}:STATe
- :LTESt:ACQuire:SWAVeform:CMODe{N}:WMEMory WMEMory{1:8}
- :LTESt:ACQuire:SWAVeform:DIFF{N}:FNAMe
- :LTESt:ACQuire:SWAVeform:DIFF:FTYPe
- :LTESt:ACQuire:SWAVeform:DIFF{N}:STATe
- :LTESt:ACQuire:SWAVeform:DIFF{N}:WMEMory
- :LTESt:ACQuire:SWAVeform:FUNCtion{N}:FNAMe
- :LTESt:ACQuire:SWAVeform:FUNCtion{N}:STATe
- :LTESt:ACQuire:SWAVeform:FUNCtion{N}:WMEMory
- :LTESt:ACQuire:SWAVeform:RESet

## Command Syntax

    :LTESt:ACQuire:SIMage:STATe {ON | OFF | 1 | 0}

## Query Syntax

    :LTESt:ACQuire:SIMage:STATe?

## Query Response

    {1 | 0}

## Description

Selects to save a screen image to a file after the limit test acquires the specified number of waveforms, samples, or patterns. Use the `:LTESt:ACQuire:CTYPe` command and its `:WAVeforms`, `:SAMPles`, or `:PATTerns` child commands to specify the test conditions required to end the test. Use the commands shown in the following table to configure the output file.

Commands to Configure the Output
Task | Command
--- | ---
Enter the filename and path | `:LTESt:ACQuire:SIMage:FNAMe`
Enter the graphics file type | `:LTESt:ACQuire:SIMage:FTYPe?`
Select portion of Infiniium display to capture | `:LTESt:ACQuire:SIMage:WINDow`
Include metadata in jpg and tiff files. | `:LTESt:ACQuire:SIMage:IMETadata`
Invert background color | `:LTESt:ACQuire:SIMage:INVert`
Black and white output | `:LTESt:ACQuire:SIMage:MONochrome`
Capture a single waveform among several displayed waveforms | `:LTESt:ACQuire:SIMage:SINClude`