# CGGS Eye Database (.cgsi)

## CGGS Format Eye Database Files

This file format is the color-grade/gray scale database (.cgsi) as an XML file comprised of an ASCII XML elements and values with the waveform data in binary.

## Example Internal Format File (.cgsi)

    <?xml version="1.0" encoding="utf-8"?>
    <InfiniiumFile>
      <Header>
        <FileType>Database</FileType>
        <Revision>1</Revision>
        <Instrument>D9300A</Instrument>
        <SwVersion>P.26.00.676</SwVersion>
        <SerialNumber>MXL3441NC2</SerialNumber>
        <Date>
          <dateTime>2025-12-05T10:37:34.5807214-07:00</dateTime>
        </Date>
      </Header>
      <PeakHits>99993</PeakHits>
      <PeakCol>524</PeakCol>
      <PeakRow>192</PeakRow>
      <TotalHits>1397616104</TotalHits>
      <NumWaves>6842</NumWaves>
      <MaxRow>845</MaxRow>
      <MinRow>177</MinRow>
      <SourceName>Channel 1 Eye</SourceName>
      <XUnits>Second</XUnits>
      <YUnits>Volt</YUnits>
      <XOrg>-3.3670044E-10</XOrg>
      <XStop>3.3670044E-10</XStop>
      <XInc>5.265057701329164E-13</XInc>
      <YBottom>-0.4</YBottom>
      <YTop>0.4</YTop>
      <YInc>0.0007820136852394917</YInc>
      <Bandwidth>60000000000</Bandwidth>
      <Status />
      <SignalType>Unspecified</SignalType>
      <SymbolRate>2969999100</SymbolRate>
      <IntrinsicNoise>0.002</IntrinsicNoise>
      <IntrinsicJitter>1E-13</IntrinsicJitter>
      <Resolution>1.220703125E-05</Resolution>
      <NumUi>2025232</NumUi>
      <Data Lengths="1280,1024">
    …………</Data>
    </InfiniiumFile>

## More Information

- Waveforms
- Main topic for Waveforms and Memory