# :FUNCtion:PARameters:FFT:WINDow

FFT Parameters Commands

- :FUNCtion:PARameters:FFT:AIMPedance
- :FUNCtion:PARameters:FFT:DETector:COUNt
- :FUNCtion:PARameters:FFT:DETector:TYPE
- :FUNCtion:PARameters:FFT:DISPlay
- :FUNCtion:PARameters:FFT:NFRequency
- :FUNCtion:PARameters:FFT:PEAK:ASCii:FDATa?
- :FUNCtion:PARameters:FFT:PEAK:ASCii:MDATa?
- :FUNCtion:PARameters:FFT:PEAK:COUNt
- :FUNCtion:PARameters:FFT:PEAK:DOUBle:FDATa?
- :FUNCtion:PARameters:FFT:PEAK:DOUBle:MDATa?
- :FUNCtion:PARameters:FFT:PEAK:ENABle
- :FUNCtion:PARameters:FFT:PEAK:LEVel
- :FUNCtion:PARameters:FFT:PEAK:SORT
- :FUNCtion:PARameters:FFT:PREFerence
- :FUNCtion:PARameters:FFT:PREFerence:TORigin
- :FUNCtion:PARameters:FFT:RBANdwidth?
- :FUNCtion:PARameters:FFT:RIMPedance
- :FUNCtion:PARameters:FFT:TFACtor
- :FUNCtion:PARameters:FFT:WINDow

## Command Syntax

    :FUNCtion{1:64}:PARameters:FFT:WINDow {RECTangular | HANNing | FTOP | BHARris | HAMMing}

Where N identifies one of up to 64 possible operators {1:64} that can be defined as part of a math function. The operators are numbered in the order that they were originally added to the function.

## Query Syntax

    :FUNCtionN:PARameters:FFT:WINDow?

## Description

Selects the shaping window to an FFT operator (`:FUNCtion:FOPerator`). You can select from Rectangular, Hanning, Flat Top, Blackman-Harris, or Hamming.

## Example Command Sequence

    :FUNCtion2:FOPerator FFT
    :FUNCtion2:PARameters:FFT:DISPlay DBM
    :FUNCtion2:PARameters:FFT:WINDow HANNing
    :FUNCtion2:COLor TCOLor4
    :FUNCtion2:DISPlay ON
    *OPC?
    …  //  Your code to synchronize execution timing.