# :LTESt:MTESt:SIMage:FTYPe?

:LTESt Mask Limit Commands

- :LTESt:MTESt:MRESult{N}:CTYPe
- :LTESt:MTESt:MRESult{N}:CTYPe:UINTervals
- :LTESt:MTESt:MRESult{N}:CTYPe:WAVeforms
- :LTESt:MTESt:MRESult{N}:SOFailure
- :LTESt:MTESt:MRESult{N}:STATe
- :LTESt:MTESt:SIMage:FNAMe
- :LTESt:MTESt:SIMage:FNAMe:AUPDate
- :LTESt:MTESt:SIMage:FNAMe:USTandard
- :LTESt:MTESt:SIMage:FTYPe?
- :LTESt:MTESt:SIMage:IMETadata
- :LTESt:MTESt:SIMage:INVert
- :LTESt:MTESt:SIMage:MONochrome
- :LTESt:MTESt:SIMage:SINClude
- :LTESt:MTESt:SIMage:STATe
- :LTESt:MTESt:SIMage:WINDow
- :LTESt:MTESt:SWAVeform:CHANnel{N}:FNAMe
- :LTESt:MTESt:SWAVeform:CHANnel:FTYPe
- :LTESt:MTESt:SWAVeform:CHANnel{N}:STATe
- :LTESt:MTESt:SWAVeform:CHANnel{N}:WMEMory
- :LTESt:MTESt:SWAVeform:CMODe{N}:FNAMe
- :LTESt:MTESt:SWAVeform:CMODe:FTYPe
- :LTESt:MTESt:SWAVeform:CMODe{N}:STATe
- :LTESt:MTESt:SWAVeform:CMODe{N}:WMEMory
- :LTESt:MTESt:SWAVeform:DIFF{N}:FNAMe
- :LTESt:MTESt:SWAVeform:DIFF:FTYPe
- :LTESt:MTESt:SWAVeform:DIFF{N}:STATe
- :LTESt:MTESt:SWAVeform:DIFF{N}:WMEMory
- :LTESt:MTESt:SWAVeform:FUNCtion{N}:FNAMe
- :LTESt:MTESt:SWAVeform:FUNCtion{N}:STATe
- :LTESt:MTESt:SWAVeform:FUNCtion{N}:WMEMory
- :LTESt:MTESt:SWAVeform:RESet

## Query Syntax

    :LTESt:MTEStN:SIMage:FTYPe?

Where N identifies a specific mask and must be a value from 1 to 16 {1:16}. For example, `:MTESt2` selects mask 2.

## Query Response

     {BITM | JPG | GIF | TIFF | PNG}

## Description

Returns the graphics file format of the last screen image file saved as a result of an measurement limit test. The file type saved is determined by the filename extension that is provided when specifying the filename using the `:LTESt:MTESt:SIMage:FNAMe` command. The following responses are returned:

`BITM`
  Bitmap (.bmp extension). A 24-bit color bitmap file format which is typically used for storing bit-mapped graphic files.
`PNG`
  The Portable Network Graphics format is a bitmap graphics file that has no compression loss and is used extensively in web pages and digital photography.
`JPG`
  A 24-bit color Joint Photographic Experts Group graphics file format (.jpg extension) that can be highly compressed. This is the default format. The image compression can result in permanent loss of image quality. The application uses the .jpg software written by the Independent JPEG Group.
`GIF`
  Graphics Interchange File format (.gif extension) is a standard graphics format (256 color) used to store bit mapped graphic files. For .gif files, this application uses LZW compression/decompression licensed under U.S. patent No 4,558,302 and foreign counterparts. The purchase or use of LZW graphics capability in a licensed product does not authorize or permit an end user to use any other product or perform any other method or activity involving use of LZW unless the end user is separately licensed in writing by Unisys. End user should not modify, copy, or distribute LZW compression/decompression capability
`TIFF`
  The 24-bit color Tag Image File format (.tif extension) is a format of choice for storing images with lossless compression. It provides better quality, but larger files. This format is widely supported across platforms (PC, Mac, UNIX). This application uses LZW compression/decompression licensed under U.S. patent No 4,558,302 and foreign counterparts. The purchase or use of LZW graphics capability in a licensed product does not authorize or permit an end user to use any other product or perform any other method or activity involving use of LZW unless the end user is separately licensed in writing by Unisys. End user should not modify, copy, or distribute LZW compression/decompression capability.