# :DISPlay:ZOOM:SOURce

:DISPlay General Commands

- :DISPlay:BLAYout
- :DISPlay:BWRap
- :DISPlay:CGSPectrum
- :DISPlay:CONNect
- :DISPlay:CTHeme
- :DISPlay:DAFFinity
- :DISPlay:DATA?
- :DISPlay:EXTHw:DMODe
- :DISPlay:FMODe
- :DISPlay:GPERformance?
- :DISPlay:GSSPectrum
- :DISPlay:HMToolbar
- :DISPlay:LOCation:A{N}:AWINdow
- :DISPlay:LOCation:A{N}:OWINdows?
- :DISPlay:LOCation:B{N}:AWINdow
- :DISPlay:LOCation:B{N}:OWINdows?
- :DISPlay:LOCation:C{N}:AWINdow
- :DISPlay:LOCation:C{N}:OWINdows?
- :DISPlay:LOCation:D{N}:AWINdow
- :DISPlay:LOCation:D{N}:OWINdows?
- :DISPlay:MARKer:DELTas
- :DISPlay:MDISplay:DOCK
- :DISPlay:MULTitouch:STATe
- :DISPlay:PSIZe
- :DISPlay:SKEYboard
- :DISPlay:SPPanel
- :DISPlay:SWINdows:INVert:STATe
- :DISPlay:TOUCh:STATe
- :DISPlay:UISCaling
- :DISPlay:VKSignal
- :DISPlay:WINTensity
- :DISPlay:ZOOM
- :DISPlay:ZOOM:SOURce

## Command Syntax

    :DISPlay:ZOOM:SOURce {CHANnel{N} | DIFF{1:4} | WMEMory{1:8}}

{N} identifies a specific channel in the form "<connection1-8>_<ch1-8>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1-8>". For example, connection 4 channel 2 is CHANnel4_2.

## Query Syntax

    :DISPlay:ZOOM:SOURce?

## Description

When the user interface Zoom Display is ON (see `:DISPlay:ZOOM`), this command specifies the waveform source that appears in the Zoom Display.