# :LTESt:MEASure:MLIMit:SOURce:TYPE

:LTESt Measurement Setup Commands

- :LTESt:MEASure:MLIMit:CFMargin
- :LTESt:MEASure:MLIMit:CFResults
- :LTESt:MEASure:MLIMit:FREGion
- :LTESt:MEASure:MLIMit:LLIMit
- :LTESt:MEASure:MLIMit:SOFailure
- :LTESt:MEASure:MLIMit:SOURce:LOCation
- :LTESt:MEASure:MLIMit:SOURce:TYPE
- :LTESt:MEASure:MLIMit:STATe
- :LTESt:MEASure:MLIMit:ULIMit
- :LTESt:MEASure:MLIMit:UPACtion

## Command Syntax

    :LTESt:MEASure:MLIMitN:SOURce:TYPE <measurement panel>

Where <measurement panel> can be: {`CRECovery{1:16}` | `EYE` | `IEEE` | `LEVel` | `MTESt{1:16}` | `OSCilloscope` | `NONE`}

Where N identifies one of sixteen {1:16} limit tests. For example, `:MLIMit8`.

## Query Syntax

    :LTESt:MEASure:MLIMitN:SOURce:TYPE?

## Description

For the specified measurement limit test 1 through 16, selects the displayed measurement panel from which to select the measurement using the `:LTESt:MEASure:MLIMit:SOURce:LOCation` command. The following table allows you to look up the proper command argument based on

- Instrument mode,
- Displayed measurement panel, and
- Waveform type.

If no measurements are turned on, `NONE` is the only valid argument and the query response. Use the `:LTESt:MEASure:MLIMit:STATe` command to enable the limit test. The measurement panel must be displayed before you can select it.

Command Argument Versus Measurement Panel
Measurement Panel | Waveform | Argument
--- | --- | ---
NRZ | PAM4
Results | ♦ | ♦ | `OSCilloscope`
Results | ♦ | ♦ | `EYE`
Mask Test | ♦ |  | `MTESt{1:16}`

## Example Command Sequence

This example returns the location of the rise time measurement, which in this example is "3". Then, later in the program, this location index is used to enable limit testing on the rise time measurement.

    :MEASure:EYE:RTIMe:LOCation?  //  Discover risetime location in table.……
    :LTESt:MEASure:MLIMit2:SOURce:TYPE EYE  //  Select an Eye test.
    :LTESt:MEASure:MLIMit2:SOURce:LOCation 3  //  Select the risetime measurement.
    :LTESt:MEASure:MLIMit2:STATe ON  //  turn on risetime limit test 2