# :MEASure:CLOCk:CTIerror:TIEFilter:DFACtor

Clock TIE Commands

- :MEASure:CLOCk:CTIerror
- :MEASure:CLOCk:CTIerror:EDIRection
- :MEASure:CLOCk:CTIerror:FAVorite
- :MEASure:CLOCk:CTIerror:LOCation?
- :MEASure:CLOCk:CTIerror:OCCurrences
- :MEASure:CLOCk:CTIerror:REGion
- :MEASure:CLOCk:CTIerror:SOURce
- :MEASure:CLOCk:CTIerror:STATus?
- :MEASure:CLOCk:CTIerror:STATus:DETails?
- :MEASure:CLOCk:CTIerror:STATus:REASon?
- :MEASure:CLOCk:CTIerror:TIEFilter
- :MEASure:CLOCk:CTIerror:TIEFilter:DFACtor
- :MEASure:CLOCk:CTIerror:TIEFilter:SHAPe
- :MEASure:CLOCk:CTIerror:TIEFilter:STARt
- :MEASure:CLOCk:CTIerror:TIEFilter:STOP
- :MEASure:CLOCk:CTIerror:TIEFilter:TYPE
- :MEASure:CLOCk:CTIerror:UNITs
- :MEASure:CLOCk:CTIerror:UREFerence:STATe
- :MEASure:CLOCk:CTIerror:UREFerence:VALue

## Command Syntax

    :MEASure:CLOCk:CTIerror:TIEFilter:DFACtor <damping_factor>

<damping_factor> is a double.

## Query Syntax

    :MEASure:CLOCk:CTIerror:TIEFilter:DFACtor?

## Description

When the Second Order TIE filter edge shape is selected (see `:MEASure:CLOCk:CTIerror:TIEFilter:SHAPe`), you can also specify the Damping Factor:

< 1 | underdamped
> 1 | overdamped
= 1.0 | critically damped
= 0.707 | Often considered ideal or optimal because of its fast settling time (optimally flat) and Butterworth type response.