# :WMEMory:CRECovery:TOPLl:DFACtor

:WMEMory CRECovery Commands

- :WMEMory CRECovery Commands
- :WMEMory:CRECovery:CEALgorithm
- :WMEMory:CRECovery:CEIDle
- :WMEMory:CRECovery:CFRequency:EDIRection
- :WMEMory:CRECovery:CFRequency:MODE
- :WMEMory:CRECovery:CSKew
- :WMEMory:CRECovery:CSRate?
- :WMEMory:CRECovery:DDRFive:CAFLatency
- :WMEMory:CRECovery:DDRFive:CAFSource
- :WMEMory:CRECovery:DDRFive:DQSSource
- :WMEMory:CRECovery:DDRFive:POLength
- :WMEMory:CRECovery:DDRFive:PRLength
- :WMEMory:CRECovery:DDRFive:RWMode
- :WMEMory:CRECovery:DDRFive:STDDelay
- :WMEMory:CRECovery:DREMoval
- :WMEMory:CRECovery:ECLock:ALIGn
- :WMEMory:CRECovery:ECLock:CFRequency
- :WMEMory:CRECovery:ECLock:CMULtiplier
- :WMEMory:CRECovery:ECLock:DELay
- :WMEMory:CRECovery:ECLock:EDIRection
- :WMEMory:CRECovery:ECLock:SOURce
- :WMEMory:CRECovery:FOPLl:LBANdwidth
- :WMEMory:CRECovery:FOPLl:LBDivisor
- :WMEMory:CRECovery:FSRate
- :WMEMory:CRECovery:MODE
- :WMEMory:CRECovery:PLL:EDIRection
- :WMEMory:CRECovery:PLL:ICCount
- :WMEMory:CRECovery:PLL:MODE
- :WMEMory:CRECovery:PLL:SSCCorrect
- :WMEMory:CRECovery:PLL:SSPercent
- :WMEMory:CRECovery:PLL:SSType
- :WMEMory:CRECovery:PLL:STIMe
- :WMEMory:CRECovery:PLL:TDEPendent
- :WMEMory:CRECovery:PRESets
- :WMEMory:CRECovery:PRESets:SELections?
- :WMEMory:CRECovery:SOPLl:JTF:LBANdwidth
- :WMEMory:CRECovery:SOPLl:JTF:LBDivisor
- :WMEMory:CRECovery:SOPLl:JTF:PEAKing
- :WMEMory:CRECovery:SOPLl:OJTF:DFACtor
- :WMEMory:CRECovery:SOPLl:OJTF:LBANdwidth
- :WMEMory:CRECovery:SOPLl:OJTF:LBDivisor
- :WMEMory:CRECovery:SRATe
- :WMEMory:CRECovery:SRATe:STATus?
- :WMEMory:CRECovery:SRATe:STATus:REASon?
- :WMEMory:CRECovery:TOPLl:DFACtor
- :WMEMory:CRECovery:TOPLl:NFReq
- :WMEMory:CRECovery:TOPLl:PFReq
- :WMEMory:CRECovery:TRACking
- :WMEMory:CRECovery:ZOPLl:LFPole
- :WMEMory:CRECovery:ZOPLl:PPOLe
- :WMEMory:CRECovery:ZOPLl:SPOLe

## Command Syntax

    :WMEMoryN:CRECovery:TOPLl:DFACtor <damping_factor>

Where N identifies one of eight {1:8} possible waveform memories. For example, `:WMEMory4`.

<damping_factor> is a double.

## Query Syntax

    :WMEMoryN:CRECovery:TOPLl:DFACtor?

## Description

Specifies the third-order PLL's damping factor (ζ).

## Example Command Sequence

    :WMEMory1:CRECovery:MODE TOPLl
    :WMEMory1:CRECovery:TOPLl:DFACtor 1.0