# :FUNCtion:PARameters:DEConvolve:BSPan?

Remove S2P Parameters Commands

- :FUNCtion:PARameters:DEConvolve:ALIGn
- :FUNCtion:PARameters:DEConvolve:BANDwidth
- :FUNCtion:PARameters:DEConvolve:BANDwidth:AUTO
- :FUNCtion:PARameters:DEConvolve:BLIMit
- :FUNCtion:PARameters:DEConvolve:BSPan?
- :FUNCtion:PARameters:DEConvolve:CFRequency
- :FUNCtion:PARameters:DEConvolve:FMODel
- :FUNCtion:PARameters:DEConvolve:FNAMe
- :FUNCtion:PARameters:DEConvolve:FRELoad
- :FUNCtion:PARameters:DEConvolve:NGAin
- :FUNCtion:PARameters:DEConvolve:PEXTract
- :FUNCtion:PARameters:DEConvolve:PORDer

## Query Syntax

    :FUNCtionN:PARameters:DEConvolve:BSPan?

Where N identifies one of up to 64 possible operators {1:64} that can be defined as part of a math function. The operators are numbered in the order that they were originally added to the function.

## Query Response

<frequency_span> is a double.

## Description

When the `BANDpass` filter type is selected (see `:FUNCtion:PARameters:DEConvolve:BLIMit`), this query returns the span of the bandpass filter.