# :TRIGger:PWIDth:REND

:TRIGger Pulse Width Commands

- :TRIGger:PWIDth:MODE
- :TRIGger:PWIDth:POLarity
- :TRIGger:PWIDth:REND
- :TRIGger:PWIDth:RSTart
- :TRIGger:PWIDth:SOURce
- :TRIGger:PWIDth:WIDTh

## Command Syntax

    :TRIGger:PWIDth:REND <seconds>

<seconds> is a double.

## Query Syntax

    :TRIGger:PWIDth:REND?

## Description

In the Pulse Width trigger mode (see `:TRIGger:MODE`), when triggering when the pulse width is inside or outside a range (see `:TRIGger:PWIDth:MODE`), this command specifies the upper range of the width.