# :CALibrate:PROBe:CHANnel:VERTical:ENABled

:CALibrate Probe Commands

- :CALibrate:PROBe:CHANnel:ENABled
- :CALibrate:PROBe:CHANnel:SKEW:ENABled
- :CALibrate:PROBe:CHANnel:SKEW:STATus?
- :CALibrate:PROBe:CHANnel:SKEW:STATus:DETails?
- :CALibrate:PROBe:CHANnel:SKEW:STATus:DTEMperature?
- :CALibrate:PROBe:CHANnel:SKEW:STATus:TIME?
- :CALibrate:PROBe:CHANnel:STARt
- :CALibrate:PROBe:CHANnel:STATus?
- :CALibrate:PROBe:CHANnel:STATus:DETails?
- :CALibrate:PROBe:CHANnel:STATus:DTEMperature?
- :CALibrate:PROBe:CHANnel:STATus:TIME?
- :CALibrate:PROBe:CHANnel:VERTical:ENABled
- :CALibrate:PROBe:CHANnel:VERTical:STATus?
- :CALibrate:PROBe:CHANnel:VERTical:STATus:DETails?
- :CALibrate:PROBe:CHANnel:VERTical:STATus:DTEMperature?
- :CALibrate:PROBe:CHANnel:VERTical:STATus:TIME?

## Command Syntax

    :CALibrate:PROBe:CHANnelN:VERTical:ENABled {ENABled | DISabled}

Where N identifies a specific channel in the form "<connection1-8>_<ch1-8>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1-8>". For example, connection 4 channel 2 is `CHANnel4_2`.

## Query Syntax

    :CALibrate:PROBe:CHANnelN:VERTical:ENABled?

## Description

On the indicated channel, enables/disables the all the probe's vertical calibration.

To enable or disable the other individual probe's calibrations, see `:CALibrate:PROBe:CHANnel:SKEW:ENABled`.

To enable or disable all the probe's calibrations, see `:CALibrate:PROBe:CHANnel:ENABled`.

To run all enabled probe calibrations, see `:CALibrate:PROBe:CHANnel:STARt`.