# :MEASure:JITTer:JITTer:PJRMs?

Jitter PJ (rms) Commands

- :MEASure:JITTer:JITTer:PJRMs?
- :MEASure:JITTer:JITTer:PJRMs:STATus?
- :MEASure:JITTer:JITTer:PJRMs:STATus:DETails?
- :MEASure:JITTer:JITTer:PJRMs:STATus:REASon?

## Query Syntax

    :MEASure:JITTerN:JITTer:PJRMs?

Where N identifies one of four possible jitter/noise analyses {1:4}. For example, `JITTer4`.

## Description

Returns PJ (rms), Periodic Jitter RMS, which is the root-mean-square value of the uncorrelated periodic jitter.