# :MEASure:JITTer:NOISe:DI?

Noise DI (δ-δ) Commands

- :MEASure:JITTer:NOISe:DI?
- :MEASure:JITTer:NOISe:DI:LEVel
- :MEASure:JITTer:NOISe:DI:STATus?
- :MEASure:JITTer:NOISe:DI:STATus:DETails?
- :MEASure:JITTer:NOISe:DI:STATus:REASon?

## Query Syntax

    :MEASure:JITTerN:NOISe:DI?

Where N identifies one of four possible jitter/noise analyses {1:4}. For example, `JITTer4`.

## Description

Returns DI (δ-δ), Deterministic Interference, which is a measure of the amount of vertical interference on a signal due to deterministic causes. The value is returned for the level specified by `:MEASure:JITTer:NOISe:DI:LEVel`).