# :MEASure:ZOOM:ZMAX

Zoom to Max/Min

- :MEASure:ZOOM:LOCation
- :MEASure:ZOOM:ZMAX
- :MEASure:ZOOM:ZMIN

## Command Syntax

    :MEASure:ZOOM:ZMAX

## Description

For Trend-able time measurements, when all occurrences are being measured over the entire waveform (see the `OCCurrences` and `REGion` commands for the measurement), the `:MEASure:ZOOM:ZMAX` command will stop acquisitions if they are running, reset statistics for the most recent acquisition, and then automatically adjust the horizontal scale and position to zoom in on the occurrence with the Maximum measured value.

Use the `:MEASure:ZOOM:LOCation` command to select the measurement on which the zoom operation will take place.