# :FUNCtion:PARameters:CTLequalizer:PRESets

CTLE Parameters Commands

- :FUNCtion:PARameters:CTLequalizer:ACGain
- :FUNCtion:PARameters:CTLequalizer:BANDwidth
- :FUNCtion:PARameters:CTLequalizer:BWMode
- :FUNCtion:PARameters:CTLequalizer:DBACgain
- :FUNCtion:PARameters:CTLequalizer:DBGain
- :FUNCtion:PARameters:CTLequalizer:DEFinition
- :FUNCtion:PARameters:CTLequalizer:FZP
- :FUNCtion:PARameters:CTLequalizer:GAIN
- :FUNCtion:PARameters:CTLequalizer:GDC
- :FUNCtion:PARameters:CTLequalizer:IMPulse
- :FUNCtion:PARameters:CTLequalizer:POLE
- :FUNCtion:PARameters:CTLequalizer:PRESets
- :FUNCtion:PARameters:CTLequalizer:PRESets:SELections?
- :FUNCtion:PARameters:CTLequalizer:STEP
- :FUNCtion:PARameters:CTLequalizer:TFUNction
- :FUNCtion:PARameters:CTLequalizer:ZERO

## Command Syntax

    :FUNCtionN:PARameters:CTLequalizer:PRESets <preset name>

Where N identifies one of up to 64 possible operators {1:64} that can be defined as part of a math function. The operators are numbered in the order that they were originally added to the function.

<preset name> is a string.

## Description

Loads a previously saved settings known as a preset for a Continuous Time Linear Equalizer (CTLE) operator. The preset configures the operator to your saved settings. To query which presets are available for loading, use the `:FUNCtion:PARameters:CTLequalizer:PRESets:SELections?` query. Many factory defaults are provided.

Presets can only be saved from the operator's Setup dialog box. There is no programming command for this task.

## Example Commands

    :FUNCtion:PARameters:CTLequalizer:PRESets "OIF CEI-28G-VSR (3db)"  //  Load a factory provided preset.

    :FUNCtion:PARameters:CTLequalizer:PRESets "MyPreset"  //  Load your saved preset.

    :FUNCtion:PARameters:CTLequalizer:PRESets:SELections?  //  Get list of saved presets.

## Child Commands

- `:FUNCtion:PARameters:CTLequalizer:PRESets:SELections?`