# :HISTogram:WINDow:DEFault

:HISTogram Commands

- :HISTogram Subsystem
- :HISTogram:ASCii:DATA?
- :HISTogram:AXIS
- :HISTogram:DISPlay
- :HISTogram:HSIZe
- :HISTogram:INCRement?
- :HISTogram:INTeger:DATA?
- :HISTogram:ORIGin?
- :HISTogram:POINts?
- :HISTogram:SCALe
- :HISTogram:SOURce
- :HISTogram:VSIZe
- :HISTogram:WINDow:BORDer
- :HISTogram:WINDow:DEFault
- :HISTogram:WINDow:X
- :HISTogram:WINDow:Y

## Command Syntax

    :HISTogramN:WINDow:DEFault

This command supports the `DEFault` common child command.

Where N identifies one of four possible histograms {1:4} that you can design. For example, `:HISTogram3`.

## Description

Sets the X1, X2, Y1, and Y2 coordinates to time and amplitude values required to create a centered histogram window 8 major graticule divisions wide and 6 divisions high. The window is shown as a blue border line on the display. This default window is the same shape regardless of the type of histogram specified with the `:HISTogram:AXIS` command. The histogram window defines the region of the measurement database that is used to construct the histogram. Use the `:HISTogram:WINDow:X` and `:HISTogram:WINDow:Y` commands to create a custom window.

Default Histogram Window