# :CHANnel:EYE:WINDow:TRACking

:CHANnel EYE Commands

- :CHANnel EYE Commands
- :CHANnel:EYE:BITS
- :CHANnel:EYE:CCOunt
- :CHANnel:EYE:CURSor
- :CHANnel:EYE:CWINdow
- :CHANnel:EYE:DISPlay
- :CHANnel:EYE:PATTern
- :CHANnel:EYE:UIXPosition
- :CHANnel:EYE:UIXRange
- :CHANnel:EYE:UUNits
- :CHANnel:EYE:WINDow:COPY
- :CHANnel:EYE:WINDow:LEFT
- :CHANnel:EYE:WINDow:METHod
- :CHANnel:EYE:WINDow:RIGHt
- :CHANnel:EYE:WINDow:TRACking
- :CHANnel:EYE:WINDow:WIDTh
- :CHANnel:EYE:XPOSition
- :CHANnel:EYE:XSCale

## Command Syntax

    :CHANnelN:EYE:WINDow:TRACking  {{ON | 1} | {OFF | 0}}

Where N identifies a specific channel in the form "<connection1-8>_<ch1-8>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1-8>". For example, connection 4 channel 2 is `CHANnel4_2`.

## Query Syntax

    :CHANnelN:EYE:WINDow:TRACking?

## Query Response

    {1 | 0}

## Description

Specifies whether a signal tracks the global eye window definition or uses its own eye window definition.

The global eye window definition is set using the `:MEASure:EYE:WINDow` commands (see Eye Window Configuration Commands).

## Example Command Sequence

    :CHANnel2:EYE:WINDow:TRACking OFF
    :CHANnel2:EYE:WINDow:METHod EOPening
    :CHANnel2:EYE:WINDow:LEFT 40.0
    :CHANnel2:EYE:WINDow:RIGHt 60.0