# :MEASure:CLOCk:PPERiod:EDIRection

Period - Period Commands

- :MEASure:CLOCk:PPERiod
- :MEASure:CLOCk:PPERiod:EDIRection
- :MEASure:CLOCk:PPERiod:FAVorite
- :MEASure:CLOCk:PPERiod:LOCation?
- :MEASure:CLOCk:PPERiod:NPERiods
- :MEASure:CLOCk:PPERiod:OCCurrences
- :MEASure:CLOCk:PPERiod:REGion
- :MEASure:CLOCk:PPERiod:SOURce
- :MEASure:CLOCk:PPERiod:STATus?
- :MEASure:CLOCk:PPERiod:STATus:DETails?
- :MEASure:CLOCk:PPERiod:STATus:REASon?
- :MEASure:CLOCk:PPERiod:UREFerence:STATe
- :MEASure:CLOCk:PPERiod:UREFerence:VALue

## Command Syntax

    :MEASure:CLOCk:PPERiod:EDIRection {RISing | FALLing}

## Query Syntax

    :MEASure:CLOCk:PPERiod:EDIRection?

## Description

For the Period - Period measurement, specifies the direction of the waveform's edges to be measured: rising or falling.

## Example Command Sequence

This sequence sets up the measurement on rising edges only.

    :MEASure:CLOCk:PPERiod:SOURce CHAN1_1
    :MEASure:CLOCk:PPERiod:EDIRection RISing
    :MEASure:CLOCk:PPERiod:NPERiods 3
      //  Perform measurement
    :MEASure:CLOCk:PPERiod
    :MEASure:CLOCk:PPERiod?