# :LTESt:MEASure:SWAVeform:FUNCtion{N}:WMEMory

:LTESt Measurement Waveform Commands

- :LTESt:MEASure:SWAVeform:CHANnel{N}:FNAMe
- :LTESt:MEASure:SWAVeform:CHANnel:FTYPe
- :LTESt:MEASure:SWAVeform:CHANnel{N}:STATe
- :LTESt:MEASure:SWAVeform:CHANnel{N}:WMEMory
- :LTESt:MEASure:SWAVeform:CMODe{N}:FNAMe
- :LTESt:MEASure:SWAVeform:CMODe:FTYPe
- :LTESt:MEASure:SWAVeform:CMODe{N}:STATe
- :LTESt:MEASure:SWAVeform:CMODe{N}:WMEMory
- :LTESt:MEASure:SWAVeform:DIFF{N}:FNAMe
- :LTESt:MEASure:SWAVeform:DIFF:FTYPe
- :LTESt:MEASure:SWAVeform:DIFF{N}:STATe
- :LTESt:MEASure:SWAVeform:DIFF{N}:WMEMory
- :LTESt:MEASure:SWAVeform:FUNCtion{N}:FNAMe
- :LTESt:MEASure:SWAVeform:FUNCtion{N}:STATe
- :LTESt:MEASure:SWAVeform:FUNCtion{N}:WMEMory
- :LTESt:MEASure:SWAVeform:RESet

## Command Syntax

    :LTESt:MEASure:SWAVeform:FUNCtion{1:64}:WMEMory WMEMory{1:8}

## Query Syntax

    :LTESt:MEASure:SWAVeform:FUNCtion{1:64}:WMEMory?

## Description

Upon completion of an measurement limit test, selects a waveform memory as a destination to save a function waveform. Use the `:LTESt:MEASure:SWAVeform:DIFF{N}:STATe` command to enable and disable waveform reporting for the channel. Use the `:LTESt:MEASure:MLIMit:STATe` command to turn off the measurement limit test.