# :DISPlay:EXTHw:DMODe

:DISPlay General Commands

- :DISPlay:BLAYout
- :DISPlay:BWRap
- :DISPlay:CGSPectrum
- :DISPlay:CONNect
- :DISPlay:CTHeme
- :DISPlay:DAFFinity
- :DISPlay:DATA?
- :DISPlay:EXTHw:DMODe
- :DISPlay:FMODe
- :DISPlay:GPERformance?
- :DISPlay:GSSPectrum
- :DISPlay:HMToolbar
- :DISPlay:LOCation:A{N}:AWINdow
- :DISPlay:LOCation:A{N}:OWINdows?
- :DISPlay:LOCation:B{N}:AWINdow
- :DISPlay:LOCation:B{N}:OWINdows?
- :DISPlay:LOCation:C{N}:AWINdow
- :DISPlay:LOCation:C{N}:OWINdows?
- :DISPlay:LOCation:D{N}:AWINdow
- :DISPlay:LOCation:D{N}:OWINdows?
- :DISPlay:MARKer:DELTas
- :DISPlay:MDISplay:DOCK
- :DISPlay:MULTitouch:STATe
- :DISPlay:PSIZe
- :DISPlay:SKEYboard
- :DISPlay:SPPanel
- :DISPlay:SWINdows:INVert:STATe
- :DISPlay:TOUCh:STATe
- :DISPlay:UISCaling
- :DISPlay:VKSignal
- :DISPlay:WINTensity
- :DISPlay:ZOOM
- :DISPlay:ZOOM:SOURce

## Command Syntax

    :DISPlay:EXTHw:DMODe {ATTenuation | GAIN | DB}

## Query Syntax

    :DISPlay:EXTHw:DMODe?

## Description

This command selects the display mode for probes and external hardware: Attenuation, Gain, or Gain (dB). Displayed fields and values are shown in terms of the selected mode.

There are separate SCPI commands for modifying the settings of each mode. For example, `:CHANnel:ESCaling:ATTenuation`, `:CHANnel:ESCaling:GAIN`, or `:CHANnel:ESCaling:DB`.