# :CMODe:COLor

:CMODe General Commands

- :CMODe:COLor
- :CMODe:CWINdow
- :CMODe:DISPlay
- :CMODe:PATTern:FILE:GCODe
- :CMODe:PATTern:FILE:NAME
- :CMODe:PATTern:FILE:RELoad
- :CMODe:PATTern:INVert
- :CMODe:PATTern:KPATtern
- :CMODe:PATTern:MODE
- :CMODe:SIGNal:TYPE
- :CMODe:SNOise:CALibrate
- :CMODe:SNOise:SNValue:LEVel{0:3}?
- :CMODe:STATus?
- :CMODe:UNAMe

## Command Syntax

    :CMODeN:COLor  {TCOLor1 | TCOLor2 | … | TCOLor48}

Where N identifies a specific common-mode waveform in the form "<connection1-8>_<ch1|ch3|ch5|ch7>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1|ch3|ch5|ch7>". When two channels are paired to create a differential waveform and a common-mode waveform, the odd-numbered channel is used when specifying the waveform. For example, connection 5 common-mode waveform 3 (from the pairing of channels 3 and 4) is `CMODe5_3`.

## Query Syntax

    :CMODeN:COLor?

## Description

Selects the color used to identify a channel on the screen. Waveform color assignments are saved as part of an instrument Setup file (`:DISK:SETup:SAVE`). Waveform colors are reset to their default values by a default setup (`:SYSTem:DEFault`) or factory default (`:SYSTem:FACTory`).

Channel Colors Versus Command Arguments
Color | Argument | Color | Argument | Color | Argument | Color | Argument
--- | --- | --- | --- | --- | --- | --- | ---
| TCOLor1 |  | TCOLor2 |  | TCOLor3 |  | TCOLor4
| TCOLor5 |  | TCOLor6 |  | TCOLor7 |  | TCOLor8
| TCOLor9 |  | TCOLor10 |  | TCOLor11 |  | TCOLor12
| TCOLor13 |  | TCOLor14 |  | TCOLor15 |  | TCOLor16
| TCOLor17 |  | TCOLor18 |  | TCOLor19 |  | TCOLor20
| TCOLor21 |  | TCOLor22 |  | TCOLor23 |  | TCOLor24
| TCOLor25 |  | TCOLor26 |  | TCOLor27 |  | TCOLor28
| TCOLor29 |  | TCOLor30 |  | TCOLor31 |  | TCOLor32
| TCOLor33 |  | TCOLor34 |  | TCOLor35 |  | TCOLor36
| TCOLor37 |  | TCOLor38 |  | TCOLor39 |  | TCOLor40
| TCOLor41 |  | TCOLor42 |  | TCOLor43 |  | TCOLor44
| TCOLor45 |  | TCOLor46 |  | TCOLor47 |  | TCOLor48

To change the color of waveforms other than channels, use the following additional `:COLor` commands that are located in other subsystems:

Additional :COLor Commands
Command | Description
--- | ---
`:CHANnel:COLor` | Sets color of channel waveforms.
`:DIFF:COLor` | Sets color of differential waveforms.
`:CGMemory:COLor` | Sets color of color grade memory waveforms
`:FUNCtion:COLor` | Sets color of math function output waveforms.
`:NETWorks:TRACe:COLor` | Sets color of S-parameter waveforms.
`:WMEMory:COLor` | Sets color of waveform memories.

## Example

    :CMODe6C TCOLor4