# :MEASure:JITTer:TFILter:STATe

Jitter/Noise Advanced Setup Commands

- :MEASure:JITTer:JITTer:TFILter:DFACtor
- :MEASure:JITTer:JITTer:TFILter:SHAPe
- :MEASure:JITTer:JITTer:TFILter:STARt
- :MEASure:JITTer:JITTer:TFILter:STOP
- :MEASure:JITTer:JITTer:TFILter:TYPE
- :MEASure:JITTer:TFILter:STATe

## Command Syntax

    :MEASure:JITTerN:TFILter:STATe {ON | OFF}

Where N identifies one of four possible jitter/noise analyses {1:4}. For example, `JITTer4`.

## Query Syntax

    :MEASure:JITTerN:TFILter:STATe?

## Description

Turns on or off the display of measurement annotations on the displayed waveform. This command also affects the appearance of annotations on screen captures.

This command lets you enable or disable a TIE filter that is applied to the jitter measurements.