# :CMODe:YSCale

:CMODe Scaling Commands

- :CMODe:YBOTtom?
- :CMODe:YOFFset
- :CMODe:YRANge
- :CMODe:YSCale
- :CMODe:YSCale:FINE
- :CMODe:YTOP?
- :CMODe:YUNits

## Command Syntax

    :CMODeN:YSCale   <scale>

<scale> is a double.

Where N identifies a specific common-mode waveform in the form "<connection1-8>_<ch1|ch3|ch5|ch7>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1|ch3|ch5|ch7>". When two channels are paired to create a differential waveform and a common-mode waveform, the odd-numbered channel is used when specifying the waveform. For example, connection 5 common-mode waveform 3 (from the pairing of channels 3 and 4) is `CMODe5_3`.

## Query Syntax

    :CMODeN:YSCale?

## Description

Sets the vertical scale (units-per-division) of the selected common-mode waveform. Use the `:CMODe:YOFFset` command to change a channel's vertical offset.