# Zoom to Maximum/Minimum Measured Value

Zoom to Max/Min

- :MEASure:ZOOM:LOCation
- :MEASure:ZOOM:ZMAX
- :MEASure:ZOOM:ZMIN

For Trend-able time measurements, when all occurrences are being measured over the entire waveform (see the `OCCurrences` and `REGion` commands for the measurement), the `:MEASure:ZOOM:ZMAX` and `:MEASure:ZOOM:ZMIN` commands will stop acquisitions if they are running, reset statistics for the most recent acquisition, and then automatically adjust the horizontal scale and position to zoom in on the occurrence with the Maximum or Minimum measured value.

Use the `:MEASure:ZOOM:LOCation` command to select the measurement on which the zoom operation will take place.