# :TRIGger:QUALify:MEASure:LOCation

:TRIGger Qualify Commands

- :TRIGger:QUALify:FOQualify
- :TRIGger:QUALify:MEASure:LLIMit
- :TRIGger:QUALify:MEASure:LOCation
- :TRIGger:QUALify:MEASure:REGion
- :TRIGger:QUALify:MEASure:ULIMit
- :TRIGger:QUALify:MODE
- :TRIGger:QUALify:STATe
- :TRIGger:QUALify:ZONE:ISZLogic
- :TRIGger:QUALify:ZONE:ZONE{N}:LOGic
- :TRIGger:QUALify:ZONE:ZONE{N}:SOURce
- :TRIGger:QUALify:ZONE:ZONE{N}:STATe
- :TRIGger:QUALify:ZONE:ZONE{N}:X
- :TRIGger:QUALify:ZONE:ZONE{N}:Y

## Command Syntax

    :TRIGger:QUALify:MEASure:LOCation  <measurement_source>

Where <measurement_source> is the number of the measurement according to the top-to-bottom order in the Measurement results window.

## Query Syntax

    :TRIGger:QUALify:MEASure:LOCation?

## Description

For measurement qualified triggers (see `:TRIGger:QUALify:MODE`), this command selects the measurement whose results are used to qualify triggers.

Use the `:TRIGger:QUALify:MEASure:LLIMit` and `:TRIGger:QUALify:MEASure:ULIMit` commands to specify the lower and upper measurement result limits.

Use the `:TRIGger:QUALify:MEASure:REGion` command to specify whether results inside or outside the limits are used to qualify triggers.