# :MEASure:CLOCk:PPWidth:STATus:DETails?

Pulse Width - Pulse Width Commands

- :MEASure:CLOCk:PPWidth
- :MEASure:CLOCk:PPWidth:FAVorite
- :MEASure:CLOCk:PPWidth:LOCation?
- :MEASure:CLOCk:PPWidth:PTYPe
- :MEASure:CLOCk:PPWidth:OCCurrences
- :MEASure:CLOCk:PPWidth:REGion
- :MEASure:CLOCk:PPWidth:SOURce
- :MEASure:CLOCk:PPWidth:STATus?
- :MEASure:CLOCk:PPWidth:STATus:DETails?
- :MEASure:CLOCk:PPWidth:STATus:REASon?
- :MEASure:CLOCk:PPWidth:UREFerence:STATe
- :MEASure:CLOCk:PPWidth:UREFerence:VALue

## Query Syntax

    :MEASure:CLOCk:PPWidth:STATus:DETails?

## Description

Returns a string that may provide additional details for a failed `:MEASure:CLOCk:PPWidth` measurement. If the measurement was successful, a null string is returned.

For a basic description of a measurement failure, use the `:MEASure:CLOCk:PPWidth:STATus:REASon?` sibling query. Use the `:STATus?` parent query to determine if the measurement has failed.

## See Also

- Measurement Errors