# :MEASure:EYE:PAM:OVERshoot:STATus:DETails?

PAM Overshoot Commands

- :MEASure:EYE:PAM:OVERshoot
- :MEASure:EYE:PAM:OVERshoot:FAVorite
- :MEASure:EYE:PAM:OVERshoot:LOCation?
- :MEASure:EYE:PAM:OVERshoot:SOURce
- :MEASure:EYE:PAM:OVERshoot:STATus?
- :MEASure:EYE:PAM:OVERshoot:STATus:DETails?
- :MEASure:EYE:PAM:OVERshoot:STATus:REASon?
- :MEASure:EYE:PAM:OVERshoot:THRatio

## Query Syntax

    :MEASure:EYE:PAM:OVERshoot:STATus:DETails?

## Description

Returns a string that may provide additional details for a failed `:MEASure:EYE:PAM:OVERshoot` measurement. If the measurement was successful, a null string is returned.

For a basic description of a measurement failure, use the `:MEASure:EYE:PAM:OVERshoot:STATus:REASon?`. Use the `:MEASure:EYE:PAM:OVERshoot:STATus?` parent query to determine if the measurement has failed.

## See Also

- Measurement Errors