# :FUNCtion:PARameters:DEPort:DRESult

DeEmbed (4 port, 1 source) Parameters Commands

- :FUNCtion:PARameters:DEPort:ALIGn
- :FUNCtion:PARameters:DEPort:BANDwidth
- :FUNCtion:PARameters:DEPort:BLIMit
- :FUNCtion:PARameters:DEPort:BSPan?
- :FUNCtion:PARameters:DEPort:CFRequency
- :FUNCtion:PARameters:DEPort:DRESult
- :FUNCtion:PARameters:DEPort:FNAMe
- :FUNCtion:PARameters:DEPort:IMPulse
- :FUNCtion:PARameters:DEPort:MEASsim
- :FUNCtion:PARameters:DEPort:RCORr
- :FUNCtion:PARameters:DEPort:RESolution
- :FUNCtion:PARameters:DEPort:SPAN
- :FUNCtion:PARameters:DEPort:STEP

## Command Syntax

    :FUNCtionN:PARameters:DEPort:DRESult {DSRC | CMSRc}

Where N identifies one of up to 64 possible operators {1:64} that can be defined as part of a math function. The operators are numbered in the order that they were originally added to the function.

## Query Syntax

    :FUNCtionN:PARameters:DEPort:DRESult?

## Description

Selects the output type of a 4-Port, 1 Source DeEmbedding operator (`:FUNCtion:FOPerator`).

The a 4-Port, 1 Source DeEmbedding operator is for situations where the differential or common-mode signal is created prior to de-embedding.

Use the `:FUNCtion:PARameters:DEPort:BANDwidth` command to specify the function's bandwidth. Use the `:FUNCtion:PARameters:DEPort:BLIMit` command to specify a bandwidth filter. Use the `:FUNCtion:PARameters:DEPort:FNAMe` command to open an existing network file that models your test setup.

DSRC
  Extracts the differential path from a 4-port transfer function.
CMSRc
  Extracts the common-mode path from a 4-port transfer function.

## Example Command Sequence

    :FUNCtion2:FOPerator DEPort
    :FUNCtion2:PARameters:DEPort:FNAMe "C:\Users<user_name>\Documents\Keysight\Infiniium\De-Embedding Networks\DUT_4.tf4"
    :FUNCtion2:PARameters:DEPort:DRESult DSRC
    :FUNCtion2:COLor TCOLor4
    :FUNCtion2:DISPlay ON
    *OPC?
    …  //  Your code to synchronize execution timing.

## Child Commands

- `:FUNCtion:PARameters:DEPort:BANDwidth`
- `:FUNCtion:PARameters:DEPort:BLIMit`
- `:FUNCtion:PARameters:DEPort:FNAMe`