# :CGMemory:DISPlay

:CGMemory General Commands

- :CGMemory:CLEar
- :CGMemory:COLor
- :CGMemory:CWINdow
- :CGMemory:DISPlay
- :CGMemory:DSTatus?
- :CGMemory:DSTatus:REASon?
- :CGMemory:PERSistence
- :CGMemory:SIGNal:TYPE
- :CGMemory:STATus?
- :CGMemory:UNAMe
- :CGMemory:UNAMe:UFName

## Command Syntax

    :CGMemoryN:DISPlay  {ON | OFF | 1 | 0}

Where N identifies one of eight color grade memories. For example, the color grade memory 2 would be identified as :CGMemory2.

## Query Syntax

    :CGMemoryN:DISPlay?

## Query Response

    {1 | 0}

## Description

Displays or hides the indicated eye-memory waveform.