# :NETWorks:TRACe:YRANge?

:NETWorks:TRACe Scaling Commands

- :NETWorks:TRACe:XLEFt?
- :NETWorks:TRACe:XPOSition?
- :NETWorks:TRACe:XREFerence?
- :NETWorks:TRACe:XRIGht?
- :NETWorks:TRACe:XSCale?
- :NETWorks:TRACe:XUNits?
- :NETWorks:TRACe:YBOTtom?
- :NETWorks:TRACe:YOFFset?
- :NETWorks:TRACe:YRANge?
- :NETWorks:TRACe:YSCale?
- :NETWorks:TRACe:YTOP?
- :NETWorks:TRACe:YUNits?

## Query Syntax

    :NETWorks:TRACeN:YRANge?

Where N identifies a specific trace and must be selected from 1 to 128 {1:128}.

## Description

Queries the trace graph's vertical range (sensitivity). This is the vertical scale per division value (`:NETWorks:TRACe:YSCale?`) multiplied by eight divisions.

Use the `:NETWorks:TRACe:YOFFset?` command to set or query the value at the center of the vertical axis.

You can query the value at the top of the graph using the `:NETWorks:TRACe:YTOP?` command.

You can query the value at the bottom of the graph using the `:NETWorks:TRACe:YBOTtom?` command.

Units for Displayed Content Window Graphs
Content Window Graphs | Y-Axis Units | X-Axis Units
--- | --- | ---
S-Parameters
Freq-Mag | Decibels | Hertz
Phase | Degrees
GrpDelay | Seconds