# :CHANnel:PROBe:HEAD:ADAPter:ID?

:CHANnel Probe Head Commands

- :CHANnel:PROBe:HEAD:ADAPter:ID?
- :CHANnel:PROBe:HEAD:ADAPter:STATe?
- :CHANnel:PROBe:HEAD:SELect
- :CHANnel:PROBe:HEAD:STATe?

## Query Syntax

    :CHANnelN:PROBe:HEAD:ADAPter:ID?

Where N identifies a specific channel in the form "<connection1-8>_<ch1-8>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1-8>". For example, connection 4 channel 2 is `CHANnel4_2`.

## Description

When a probe head adapter is connected (see `:CHANnel:PROBe:HEAD:ADAPter:STATe?`), this query returns the model number of the probe head adapter.