# :NETWorks:TRACe:UNAMe?

:NETWorks:TRACe General Commands

- :NETWorks:TRACe:COLor
- :NETWorks:TRACe:CWINdow
- :NETWorks:TRACe:DISPlay
- :NETWorks:TRACe:NETWork
- :NETWorks:TRACe:OPERator
- :NETWorks:TRACe:PARameter
- :NETWorks:TRACe:STATus?
- :NETWorks:TRACe:UNAMe?

## Query Syntax

    :NETWorks:TRACeN:UNAMe?

Where N identifies a specific trace and must be selected from 1 to 128 {1:128}.

## Description

This command queries the S-parameter name of a trace waveform.

User names are displayed on the screen.