# NRZ Eye Measurements

Measurements

- Time Measurements
- Amplitude Measurements
- Clock Measurements
- Data Measurements
- SNDR Measurements
- PAM Measurements
- FFT Measurements
- User-Defined Measurements
- NRZ Eye Measurements
- PAM Eye Measurements
- Mask Test Commands
- Querying Measurement Results and Statistics

`:MEASure:EYE`

- :MEASure:EYE:AMPLitude (Eye Amplitude)
- :MEASure:EYE:BITRate (Bit Rate)
- :MEASure:EYE:CROSsing (Crossing %)
- :MEASure:EYE:DCDistortion (Duty Cycle Distortion)
- :MEASure:EYE:DTIMe (Δ Time)
- :MEASure:EYE:ECTime (Crossing Time)
- :MEASure:EYE:EHEight (Eye Height)
- :MEASure:EYE:ESN (Signal to Noise Ratio)
- :MEASure:EYE:EWIDth (Eye Width)
- :MEASure:EYE:FTIMe (Fall Time)
- :MEASure:EYE:JITTer (Jitter)
- :MEASure:EYE:OLEVel (One Level)
- :MEASure:EYE:PEAK (Database Peak Hits)
- :MEASure:EYE:RTIMe (Rise Time)
- :MEASure:EYE:ZLEVel (Zero Level)