# :MEASure:THReshold:GENeral:MIDDle

Threshold Definition Commands

- :MEASure:TBASe:GENeral:BASE
- :MEASure:TBASe:GENeral:METHod
- :MEASure:TBASe:GENeral:TOP
- :MEASure:TBASe:RFALl:BASE
- :MEASure:TBASe:RFALl:METHod
- :MEASure:TBASe:RFALl:TOP
- :MEASure:THReshold:EREFerence
- :MEASure:THReshold:GENeral:HYSTeresis
- :MEASure:THReshold:GENeral:LOWer
- :MEASure:THReshold:GENeral:METHod
- :MEASure:THReshold:GENeral:MIDDle
- :MEASure:THReshold:GENeral:PLOWer
- :MEASure:THReshold:GENeral:PMIDdle
- :MEASure:THReshold:GENeral:PUPPer
- :MEASure:THReshold:GENeral:UPPer
- :MEASure:THReshold:PAM:GENeral:HYSTeresis
- :MEASure:THReshold:PAM:GENeral:LMEThod
- :MEASure:THReshold:PAM:GENeral:METHod
- :MEASure:THReshold:PAM:GENeral:PAMLevel:LEVel{N}
- :MEASure:THReshold:PAM:GENeral:THResholds:EYE{N}
- :MEASure:THReshold:PAM:RFALl:LMEThod
- :MEASure:THReshold:PAM:RFALl:METHod
- :MEASure:THReshold:PAM:RFALl:PAMLevel:LEVel{N}
- :MEASure:THReshold:RFALl:LOWer
- :MEASure:THReshold:RFALl:METHod
- :MEASure:THReshold:RFALl:PLOWer
- :MEASure:THReshold:RFALl:PUPPer
- :MEASure:THReshold:RFALl:UPPer

## Command Syntax

    :MEASure:THReshold:GENeral:MIDDle  <amplitude>

Where <amplitude> is a double.

## Query Syntax

    :MEASure:THReshold:GENeral:MIDDle?

## Description

Sets or queries the global middle threshold-definition level. This value is used when making measurements with custom threshold definitions that are based on absolute amplitude. When custom threshold definitions are based on percent, use the `:MEASure:THReshold:GENeral:PMIDdle` command.

Use the `:MEASure:THReshold:GENeral:METHod` command to set waveform threshold levels to standard percentages or custom definitions.

Use the `:MEASure:THReshold:GENeral:UPPer` command to enter a upper threshold level. Use the `:MEASure:THReshold:GENeral:LOWer` command to enter a lower threshold level.

## Example Command Sequence

    :MEASure:THReshold:GENeral:METHod ABSolute
    :MEASure:THReshold:GENeral:UPPer 125E-3
    :MEASure:THReshold:GENeral:MIDDle 0E0
    :MEASure:THReshold:GENeral:LOWer -125E-3