# <Resolution> Element

The <Resolution> element sets a resolution for a <Double> User-Defined Control to the User Operator Setup dialog box. The resolution is based on the unit of measurement (without multiplier). For example, in the following picture a "1000" resolution specifies that the value of Fc can be set to a minimum resolution of 1000 Hz. Therefore, using keyboard entry 7.500000 GHz can be changed to 7.500001 GHz. A setting of 1000000 would have limited the resolution to 1 MHz. <Resolution> does not affect the step sizes of the step buttons.

- XML file elements

## Parent Elements

- <Double>

## Child Elements

None

## Attributes

None

## Example

- <Function>
- …
- <Control Name = "Fc">
- <Double>
- <Min>10e6</Min>
- <Max>1000e9</Max>
- <Resolution>1000</Resolution>
- <Units>Hertz</Units>
- <Default>7.5e9</Default>
- </Double>
- …
- </Function>