# :WMEMory:EYE:UUNits

:WMEMory EYE Commands

- :WMEMory EYE Commands
- :WMEMory:EYE:BITS
- :WMEMory:EYE:CCOunt
- :WMEMory:EYE:CURSor
- :WMEMory:EYE:CWINdow
- :WMEMory:EYE:DISPlay
- :WMEMory:EYE:PATTern
- :WMEMory:EYE:UIXPosition
- :WMEMory:EYE:UIXRange
- :WMEMory:EYE:UUNits
- :WMEMory:EYE:WINDow:COPY
- :WMEMory:EYE:WINDow:LEFT
- :WMEMory:EYE:WINDow:METHod
- :WMEMory:EYE:WINDow:RIGHt
- :WMEMory:EYE:WINDow:TRACking
- :WMEMory:EYE:WINDow:WIDTh
- :WMEMory:EYE:XPOSition
- :WMEMory:EYE:XSCale

## Command Syntax

    :WMEMoryN:EYE:UUNits {UINTerval | SECond}

Where N identifies one of eight {1:8} possible waveform memories. For example, `:WMEMory4`.

## Query Syntax

    :WMEMoryN:EYE:UUNits?

## Query Response

    {UINT | SEC}

## Description

This command specifies the user interface's units option for the real-time eye horizontal Scale and Position controls. You can select either Unit Intervals (UIs) or time (in seconds).

To specify the real-time eye horizontal scale and position in terms of UI units, use the `:WMEMory:EYE:UIXRange` and `:WMEMory:EYE:UIXPosition` commands.

To specify the real-time eye horizontal scale and position in terms of time units, use the `:WMEMory:EYE:XSCale` and `:WMEMory:EYE:XPOSition` commands.