# :MEASure:JITTer:JITTer:RJ?

Jitter RJ (rms) Commands

- :MEASure:JITTer:JITTer:RJ?
- :MEASure:JITTer:JITTer:RJ:STATus?
- :MEASure:JITTer:JITTer:RJ:STATus:DETails?
- :MEASure:JITTer:JITTer:RJ:STATus:REASon?

## Query Syntax

    :MEASure:JITTerN:JITTer:RJ?

Where N identifies one of four possible jitter/noise analyses {1:4}. For example, `JITTer4`.

## Description

Returns RJ (rms), Random Jitter, which is the root-mean-square value of the Gaussian-shaped component of the total jitter.

The measurement shows "rms,wide" or "rms,narrow", depending on the `:MEASure:JITTer:JITTer:RJBandwidth` setting.