# :WMEMory:FILE:LOAD

:WMEMory Loading Commands

- :WMEMory:LOAD
- :WMEMory:LOAD:SOURce
- :WMEMory:FILE:LOAD
- :WMEMory:FILE:NAME

## Command Syntax

    :WMEMoryN:FILE:LOAD

Where N identifies one of eight {1:8} possible waveform memories. For example, `:WMEMory4`.

## Description

Loads the selected waveform file (.h5, .csv, or .txt) into the indicated waveform memory location. Use the `:WMEMory:FILE:NAME` command to specify the name of the file to load. Use the `:WMEMory:DISPlay` command to display the waveform memory.

To load a waveform source into memory, for example connection 1 channel 1, use the `:WMEMory:LOAD` command.