# :WAVeform:CGRade:STATus:REASon?

:WAVeform CGRade Commands

- :WAVeform:CGRade:ASCii:DATA?
- :WAVeform:CGRade:COLumns?
- :WAVeform:CGRade:INTeger:DATA?
- :WAVeform:CGRade:POINts?
- :WAVeform:CGRade:ROWS?
- :WAVeform:CGRade:STATus?
- :WAVeform:CGRade:STATus:REASon?
- :WAVeform:CGRade:UICount?
- :WAVeform:CGRade:WCOunt?
- :WAVeform:CGRade:XINCrement?
- :WAVeform:CGRade:XML:READ?
- :WAVeform:CGRade:XML:WRITe?
- :WAVeform:CGRade:XORigin?
- :WAVeform:CGRade:YINCrement?
- :WAVeform:CGRade:YORigin?

## Query Syntax

    :WAVeform:CGRade:STATus:REASon?

## Description

Queries a string that explains why the `:WAVeform:CGRade:STATus?` parent command indicates invalid or questionable waveform data. The following strings may be returned by this query:

""
  A null string indicates that the data is correct.
"Clipped Hi"
  The amplitude of the waveform is too large and the data is clipped off the top of the screen.
"Clipped Low"
  The amplitude of the waveform is too large and the data is clipped off the bottom of the screen.

## Parent Command

- `:WAVeform:CGRade:STATus?`